
Anexa 6.1.1 – Specificatii tehnice (B/S)
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Achiziția de BUNURI

	Denumirea achiziției: BUNURI (Laptop, dronă) pentru anul IV de proiect



	
	Specificații tehnice solicitate

	Lot 1 – Laptop

	1
	Denumire produs: Laptop

	
	Descriere generala:
Laptop, processor cu 8 core, 16 fire de executie, min. 24 MB Cache, frecventa turbo min. 4,9 GHz, frecventa baza min. 2,1 GHz, SSD 1TB PCI expres, Memorie RAM DDR4 – min 16GB, placa video dedicata min 8GB, porturi conectivitate: 1 x Mini DisplayPort, 1 x HDMI, 1 x RJ-45, 1 x Audio Out/Microfon, 3 x USB 3.2 Type A Gen 1, 1 x port ce permite viteza de transfer de min. 40 Gbps, Wireless, Bluetooth, display QHD min 17”, tehnologie display IPS, webcam integrata
Termen de garantie min. 2 ani

	2
	Denumire produs: Tricou personalizat 

	Lot 2 – Dronă

	1
	Denumire produs: Drona

	
	Descriere generala: 
Drona dotată cu două camera,  Fotografii de 20MP, Dynamic range – 12.8 stopuri, Diafragma reglabila – f/2.8-f/11, Distanta focala echivalenta de 24mm, VDAF – Vision Detection Auto Focus Technology, Timp de zbor extins de 46 de minute, Interval de transmisie video de 15km, Feed live FHD 1080p@60fps, Tehnologie de pozitionare cu precizie extrema, Inregistrare video 5.1K, DCI 4K@120fps, Apple ProRes 422 HQ, D-Log pe 10 biti, Greutate de decolare 501g-2kg, Culoare gri, Ttimp de zbor >35min,Distanta max. de operare >9000m,Senzori de obstacole, Omnidirectional, Greutate de baza 895g, Dimensiuni347.5×283×107.7 mm,Viteza maxima de inclinare	1 m/s (C mode); 6 m/s (N mode); 8 m/s (S mode), Viteza maxima 5 m/s (C mode); 15 m/s (N mode); 19 m/s (S mode) Altitudine maxima 6000 m,  Autonomie timp zbor: minim 46 min., Distanta maxima de operare: 30 km; Unghi maxim de inclinare 25° (C mode); 30° (N mode); 35° (S mode), Temperatura de operare	-10°C - 40°C Tip GPS GPS + Galileo + BeiDou, Acuratete de planare Vertical:±0.1 m (with Vision Positioning); ±0.5 m (with GNSS Positioning); Horizontal:±0.3 m (with Vision Positioning); ±0.5 m (with High-recision Positioning System) Memorie interna 8 GB, Tip Camera Hasselblad 4/3 CMOS, Effective pixels:20 MP, ISO Camera Hasselblad Video:100-6400; Photo:100-6400, Rezolutie Video Apple ProRes 422 HQ; 5.1K:5120×2700@24/25/30/48/50fps; DCI 4K:4096×2160@24/25/30/48/50/60/120*fps; 4K:3840×2160@24/25/30/48/50/60/120*fps; H.264/H.265; 5.1K:5120×2700@24/25/30/48/50fps; DCI 4K:4096×2160@24/25/30/48/50/60/120*fps; 4K:3840×2160@24/25/30/48/50/60/120*fps; FHD:1920×1080p@24/25/30/48/50/60/120*/200*fps
Formate suportate	Photo:JPEG/DNG (RAW); Video:MP4/MOV (MPEG-4 AVC/H.264, HEVC/H.265), Tip Tele Camera	1/2-inch CMOS
ISO Tele Camera Video:100-6400; Still Image:100-6400, Imagine Max, 4000X3000, Formate suportate	Photo:JPEG; Video:MP4/MOV (MPEG-4 AVC/H.264, HEVC/H.265), Rezolutie video Tele Camera	H264/H.265; 4K:3840×2160@30 fps; FHD:1920×1080@30 fps, Zoom Digital	4X
Stabilizare Gimbal pe 3 axe, Acuratete gimbal Tilt:-135° to 100°; Roll:-45° to 45°; Pan:-27° to 27°, Senzori de obstacole Omnidirectional, Frecvente de operare 2.400-2.4835 GHz; 5.725-5.850 GHz, Distanta emitere semnal max 15 km, Tip baterie, LiPo 4S; 5000mAh; 15.4V, Tip telecomanda  DJI RC-N1
Termen de garanție min 12 luni.



Nume, prenume: Creanga Ramona
Semnătură:
Data: ...........
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